{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":18,"n_cols":12,"rows_kept":18,"merged":[[0,0,0,11],[2,0,2,11],[17,0,18,11],[21,16,21,25]]}
["界首高新区企业服务中心发光字制作及采购项目技术参数及清单"]
[]
[]
["序号","名称","规格要求","尺寸","电压、功率","参考品牌","平方数","单位","数量","单价/元","合计/元","备注"]
[1,"火炬标志（楼顶北面）","镀锌钢板点阵字","6m*5m","24v","憨豆，蓝景、晶宏亮，三源彩",30,"个",1,null,null,"品牌&9外露穿孔灯，25mm灯间距，1.2mm厚热镀锌板，烤漆，晶元芯片，质保3年"]
[2,"界首市企业服务中心（楼顶横向）","镀锌钢板点阵字","4.5m*3.5m","24v","憨豆，蓝景、晶宏亮，三源彩",141.75,"个",9,null,null,"品牌&9外露穿孔灯，25mm灯间距，1.2mm厚热镀锌板，烤漆，晶元芯片，质保3年"]
[3,"防水电源","400W/DC12V",null,"24v","工程专用型",null,"台",40,null,null,"工程专用质保3年"]
[4,"火炬标志钢结构\n(按图纸方案含各种组成部分的斜拉撑）","国标镀锌角铁焊接","8.8m*5m",null,"天津友发、 鞍钢、马钢",44,"平方",1,null,null,"国标40*40镀锌角铁方笼焊接+镀锌方管+地脚钢板、立柱就女儿墙2道方笼钢构链接"]
[5,"横向大字钢结构\n(按图纸方案含各种组成部分的斜拉撑）","国标镀锌角铁焊接","7.5m*3.5m",null,"天津友发、 鞍钢、马钢",236,"平方",9,null,null,"国标40*40镀锌角铁方笼焊接+镀锌方管+地脚钢板、立柱就女儿墙2道方笼钢构链接"]
[6,"支撑混泥土墩子（含钢板、防水处理）","配重水泥墩子","0.8m*0.8m",{"$nulls":3},"个",20,null,null,"混凝土+人工+板材"]
[7,"电气配线","电气配线","YJV5*6m","24v","德力西、正泰、鑫源电线",200,"米","2把"]
[8,"电气配线","电气配线","RVV2*2.5m","24v","德力西、正泰、鑫源电线",800,"米","4把"]
[9,"配电箱","工程专用",null,"24v","德力西、正泰",null,"台",2]
[10,"铺材","焊条、油漆、固定件膨胀螺丝、钻尾丝  穿线管",{"$nulls":4},"项",1]
[11,"安装费",{"$nulls":4},264.5,"项",1,null,null,"焊接钢结构架+安装字排线"]
[12,"吊车","200吨",{"$nulls":4},"项",1]
[null,"总合计"]
["注意：\n\n1、每组亮化及发光字报价均含独立的配电箱、漏电保护器、定时器、国标电线等完成本项目的所有组成部分。\n\n2、报价前必须实地勘查现场，以充分了解工地位置、情况、道路、储存空间、装卸限制及任何其他足以影响报价的情况,任何因忽视或误解工地情况而导致的索赔或工期延长申请将不被批准。\n\n3、所有投标报价均包括所需人工费、施工机械使用费、材料费、以及管理费、利润、税务、其它（运杂费、质检费、安装费、高空作业保险费、以及合同明示或暗示的风险、责任和义务）等。\n\n4、严格按“界首高新区企业服务中心发光字制作及采购项目”招标文件以及参考品牌（其他品牌不低于参考品牌标准）、技术参数要求实施，详见结构施工说明以及动态、静态效果图。\n\n5、严禁贴牌高仿，灯具功率必须足瓦数，中标时需提供灯具及钢材产品检测报告。                                                            6、质保期5年。质保期内提供24小时热线服务和现场支持服务，若出现质量问题或其它情况导致设备不能正常使用的，中标人必须在接报后2小时内响应，24小时内到达现场，48小时内免费恢复设备正常使用。"]